1. Measure the diameter of the No. 1 journal on the rear balancer shaft.
   Journal Diameter
   Standard (New): | 23.938−23.950 mm
   (0.9424−0.9429 in.)
   Service Limit: | 23.92 mm (0.942 in.)
Clean both balancer shaft No. 2 journals and balancer shaft holders with a clean shop towel. Place one strip of plastigage across each No. 2 journals. Reinstall the bearings and upper balancer shaft holder, then torque the bolts. NOTE: Do not rotate the balancer shafts during inspection. |