Exploded View Special Tools Required Handle driver 07749-0010000 Driver attachment, 42 x 47 mm 07746-0010300 NOTE: Refer to the Exploded View as needed during this procedure. Test the alternator and regulator before you remove them. Remove the alternator. If the front bearing needs replacing, remove the pulley locknut with a 10 mm wrench (A) and a 22 mm wrench (B). If necessary, use an impact wrench. |