DTC B1357: Power Tailgate Control Unit Lost Communication with Gauge Control Module (VSP/NE Message) Clear the DTCs using the HDS. Cycle the ignition switch to OFF, and then back ON. Check for DTCs by selecting the DTCs MENU (DTCs) from the HDS. Are is DTC B1060, B1205, B1357 and B1610?
YES | - | Go to Step 4 .
NO | - | Faulty gauge control module; replace it.■
Check for continuity between the No. 3 and No. 5 terminals of power tailgate control unit connector B (5P) and body ground. Is there continuity?
YES | - | Faulty power tailgate control unit; replace it.■
NO | - | Repair an open in the BLK wire(s), or poor ground (G705).■