Power Mirror Replacement

Lower the door glass fully. Carefully pry out the mirror mount cover (A) by hand in the sequence shown. Remove the door panel. |

Remove the plastic cover as necessary, then detach the harness clip (A), and disconnect the connector (B). While holding the mirror (C), remove the nuts. |

Remove the mirror (A). Take care not to scratch the door. Install the mirror in the reverse order of removal, and make sure the connector is plugged in properly. |