M/T Countershaft Disassembly

Securely clamp the countershaft assembly in a bench vise with wood blocks. Remove the 20 mm special bolt (left-hand threads). |

Support the ball bearing (A) on steel blocks (B), then use a press (C) and an attachment (D) to press the countershaft (E) out of the ball bearing. Remove the 35 mm shim and distance collar. |

Support 4th gear (A) on steel blocks (B), then use a press (C) and an attachment (D) to press the countershaft (E) out of the 4th and 5th gear. |

Support 2nd gear (A) on steel blocks (B), then use a press (C) and an attachment (D) to press the countershaft (E) out of the 2nd and 3rd gear. |