Installation Connect the connectors to the under-hood fuse/relay box, then install the under-hood fuse/relay box in the reverse order of removal. Install the removed parts in the reverse order of removal. Connect the both positive cable and negative cable to the battery. Do the ECM/PCM idle learn procedure. Do the power window control unit reset procedure. Enter the anti-theft codes for the radio and navigation system, then enter the customer's radio station presets. Confirm that all systems work properly. |