Reverse idler gear

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Reverse idler gear | Reverse idler gear shaft diameter at needle bearing contact area |  | 14.99−15.00 mm (0.5902−0.5906 in.) | When worn or damaged
I.D. |  | 20.007−20.020 mm (0.7877−0.7882 in.) | When worn or damaged
I.D. of reverse idler gear shaft contact area on transmission housing |  | 14.800−14.818 mm (0.5827−0.5834 in.) | ———
I.D. of reverse idler gear shaft holder |  | 14.800−14.824 mm (0.5827−0.5836 in.) | When worn or damaged