NOTE: Do not use this troubleshooting procedure if only one fan is inoperative, or if the A/C compressor is inoperative, refer to the symptom troubleshooting index. Check the No. 9 (20 A) and No. 11 (20 A) fuses in the under-hood fuse/relay box, and the No. 30 (7.5 A) fuse in the under-dash fuse/relay box. Are the fuses OK?
YES | - | Go to Step 2 .
NO | - | Replace the fuse(s), and recheck.■
Remove the A/C condenser fan relay from the under-hood fuse/relay box. Turn the ignition switch ON (II). Measure the voltage between the No. 3 terminal of the A/C condenser fan relay 4P socket and body ground. Is there battery voltage?
YES | - | Go to Step 5 .
NO | - | Repair open in the wire between the No. 30 fuse in the under-dash fuse/relay box and the A/C condenser fan relay.■
Turn the ignition switch OFF. Reinstall the A/C condenser fan relay. Make sure the A/C switch is OFF, and the engine coolant temperature is below 93 °C (199 °F). Turn the ignition switch ON (II). |