DTC 44-2x (44-20 to 44-29, 44-2A to 44-2F),44-3x (44-30 to 44-39, 44-3A to 44-3F),44-Bx (44-B0 to 44-B9, 44-BA to 44-BF): Internal Failure of the Right Side Impact Sensor (first) Erase the DTC memory. Turn the ignition switch ON (II), and check that the SRS indicator comes on for about 6 seconds and then goes off. Does the SRS indicator stay on and is DTC 44-2x, 44-3x, or 44-Bx indicated?
YES | - | Replace the right side impact sensor (first). If the DTC returns, replace the SRS unit.■
NO | - | Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures. If another DTC is indicated, go to the DTC troubleshooting details.