DTC Troubleshooting: 31, 32, 33, 34, 35, 36, 37, 38

DTC 31, 32, 33, 34, 35, 36, 37, 38: ABS Solenoid Clear the DTC using the HDS. Turn the ignition switch ON (II). Verify the DTC. Does the ABS indicator come on, and are DTCs 31, 32, 33, 34, 35, 36, 37, and/or 38 indicated?
YES | - | Check for loose terminals in the VSA control unit 47P connector. If necessary, substitute a known-good VSA modulator-control unit, and recheck.■
NO | - | The system is OK at this time.■