VSA Sensor Cluster Replacement

NOTE: Do not damage or drop the sensor as it is sensitive. LHD type is shown, RHD type is symmetrical. Remove the driver's/passenger's center lower cover and rear vent duct. Remove the bracket mounting bolt (A) on driver's side. |

Remove the bracket mounting bolt (A) on passenger's side. Remove the connector mounting bracket (B). Remove the sensor cluster (C) with the bracket. |

Disconnect the sensor cluster connector (A). Remove the bracket (B) from the sensor cluster (C). Install in the reverse order of removal. |