Install the steering wheel bolt (A) and tighten it to the specified torque, then connect the cable reel subcord connector (B). Make sure the wire harness is routed and fastened properly. Install the driver's airbag, and confirm that the system is operating properly. Do the ECM/PCM idle learn procedure. Reset the power window control unit. For with LKAS model: Do the steering angle sensor neutral position memorization. Enter the anti-theft codes for the radio and the navigation system, then enter the customer's radio station presets. Reset the clock. Check the cruise control, audio remote, navigation guide and turn signal canceling for proper operation. |