1. Attach the upper rubber dam (A), lower side rubber dam (B), and clips (C) with adhesive tape, and attach the dashboard seal A (D) and dashboard seal B (E) to the inside face of the windshield (F) as shown: Be sure the rubber dam and clips line up with the alignment marks (G). Be sure the dashboard seals line up with the lower side rubber dam. Be careful not to touch the windshield where adhesive will be applied.
   Rubber dams adhesive tape:
   | Thickness 0.16 mm (0.0063 in.)
   | Width 3.5 mm (0.14 in.)
   Clips adhesive tape:
   | Thickness 0.4 mm (0.016 in.)
   | Width 10 mm (0.39 in.)
   Dashboard seal A adhesive tape:
   | Width 21 mm (0.83 in.)
   Dashboard seal B adhesive tape:
   | Width 12 mm (0.47 in.)