1. After installing a new set of rings, measure the ring-to-groove clearances:
   Top Ring Clearance
   Standard (New): | 0.07−0.11 mm (0.003−0.004 in.)
   Service Limit: | 0.12 mm (0.005 in.)
   Second Ring Clearance
   Standard (New): | 0.04−0.08 mm (0.002−0.003 in.)
   Service Limit: | 0.10 mm (0.004 in.)
   Oil Ring Clearance
   Standard (New): | 0.02−0.06 mm (0.001−0.002 in.)
   Service Limit: | 0.08 mm (0.003 in.)