Check for continuity between PCM connector terminals C5 and A8 or A9. Is there continuity?
YES | - | Repair short to ground in the wire between PCM connector terminal C5 and the shift solenoid harness connector, then go to Step 13 .
NO | - | Check shift solenoid valve D, and check for a short in the shift solenoid harness in the transmission. Replace shift solenoid valve D and/or shift solenoid harness, then go Step 13 .
Clear the DTC with the HDS. Start the engine, and shift the transmission in 2nd gear in the M position. Monitor the OBD status for P0982 in the DTCs/Freeze Data in A/T Mode Menu for a pass/fail. Does the result indicate a pass?
YES | - | The problem has been corrected.■
NO | - | Return to Step 1 and recheck.■