1. Install the trim in the reverse order of removal, and note these items: Replace any damaged clips with a new one. Do not reuse the rear pillar cap; always replace it. If the side curtain airbag has deployed, replace the rear pillar trim with new one. To prevent the side curtain airbags from deploying improperly and possibly causing injury, inspect removed pieces and replace them if they have any of these types of damage.
   - | Any cracks, deformations, or stress-whitenings in the rear pillar trim (A)
   - | Any cracks, or stress-whitenings in the grommet and clip seating surfaces (B)
   - | Bent or broken grommet (C)
Replace any damaged parts with new ones. Make sure the top of the trim overlaps with the headliner correctly. Push the clips into place securely. |