1st/2nd triple cone synchro

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
1st/2nd triple cone synchro | Outer synchro ring-to-synchro cone clearance | Ring pushed against gear | 0.70−1.19 mm (0.028−0.047 in.) | 0.3 mm (0.012 in.)
Synchro cone-to-gear clearance | Ring pushed against gear | 0.45−1.14 mm (0.018−0.045 in.) | 0.3 mm (0.012 in.)
Outer synchro ring-to-gear cone clearance | Ring pushed against gear | 1.12−1.68 mm (0.044−0.066 in.) | 0.6 mm (0.024 in.)