NOTE: The illustrations show LHD model, RHD model is symmetrical. Before installing the steering gearbox, make sure that no power steering fluid is on the mating surface of the gearbox and a front suspension subframe. To prevent the gearbox mounting bolts from loosening after the installation, remove the power steering fluid from the mount cushions and bolt holes. Apply a mild soap and water solution to both side of the mount cushion mating surfaces (A). Pass the cylinder of the steering gearbox (B) through the wheelwell opening on the driver's side. Carefully move the steering gearbox toward the passenger's side until the pinion shaft clears the wheelwell opening on the body. |