Remove the dipstick and check the fluid level. It should be between the upper mark (A) and lower mark (B). If the level is below the lower mark, check for fluid leaks at the transmission, and hose and line joints. If a problem is found, fix it before filling the transmission with ATF. NOTE: If the vehicle is driven when the ATF level is below the lower mark: Transmission damage will result. Vehicle does not move in any gear. Vehicle accelerates poorly, and flares when starting off in the D and R positions. The engine vibrates at idle. If the level is above the upper mark, drain the ATF to proper level. NOTE: If the vehicle is driven when the ATF level is above the upper mark, the vehicle may creep forward while in the N position, or have shifting problems. |