Check for continuity between fuel pump 5P connector terminal No. 5 and body ground. Is there continuity?
YES | - | Replace PGM-FI main relay 2 (FUEL PUMP). Also replace the No. 19 FUEL PUMP (15 A) fuse.■
NO | - | Check the fuel pump, and replace it if necessary. Also replace the No. 19 FUEL PUMP (15 A) fuse.■
Jump the SCS line with the HDS. Disconnect ECM/PCM connector E (31P). Turn the ignition switch ON (II). |