Remove the brake booster (A) from the engine compartment. Be careful not to damage the booster surfaces and threads of the booster stud bolts. Be careful not to bend or damage the brake lines. Install the brake booster in the reverse order of removal, and note these items: Tighten all mounting hardware to the specified torque values. Use a new lock pin whenever installing. After installing the brake booster and master cylinder, fill the reservoir with new brake fluid, bleed the brake system, and adjust the brake pedal height and free play. |