Turn the shift fork shaft (A) so the large chamfered hole (B) is facing the fork bolt hole (C) of the shift fork (D). Install the shift fork and reverse selector together on the shift fork shaft and countershaft. Secure the shift fork to the shift fork shaft with the lock bolt and a new lock washer (E), then bend the lock tab of the lock washer against the bolt head. Install the needle bearing and countershaft reverse gear on the countershaft. Install the reverse idler gear in the transmission housing. Install the idler gear shaft, if it was removed. |