Start-up procedure and Diagnosis Menu Turn the ignition switch ON (II), press ‘‘OK'' on the disclaimer screen, then press and hold the keys in this order: (1) MENU Key. (2) MAP/GUIDE Key, (3) CANCEL Key, and keep them pressed simultaneously for 5 seconds. After the display changes to the diagnosis menu screen, touch the item you want to check, and the check will start. To return to the previous screen, touch the ‘‘RETURN'' switch on the diagnosis screen. System Links Tire-Calibrate Monitor Check Yaw Rate Unit Check Cyclic Diag In-line Diag Vehicle Position Start Demo Mode |