1. Turning Angle Inspection Raise the vehicle and set the turning radius gauges beneath the front wheels, and place boards under the rear wheels the same thickness as the turning radius gauges, then lower the vehicle. NOTE: Be sure that the vehicle is level with the wheels on the turning radius gauges and boards. Turn the steering wheel fully to the right and left while applying the brake, and check the turning angles of both front wheels. If the turning angle is not within the specification or the inward turning angles differ between the right and left, go to Step 3 .
   Turning angle:
   | Inward: | 38 ° 50 ′±2 °
   | Outward: | 31 ° 40 ′ (reference)
Check the toe. If it is correct but the turning angle is not within the specification, check for bent or damaged suspension components. |