1. Remove the lower tailgate touch sensor (A).
   -1. | Disconnect the sensor connector (B).
   -2. | Remove the mounting bolt (C) and clip (D).
   -3. | Remove the lower tailgate touch sensor and grommet (E) from the tailgate, then pull the harness out.
Install the sensor in the reverse order of removal, and note these items: Make sure the connectors are plugged in properly. Reconnect the negative cable to the battery. Reset the clock. Perform the power window control unit reset procedure. Check the tailgate touch sensor operation. |