SRS components are located in this area. Review the SRS components locations, and the precautions, and procedures before performing repairs or service. Turn the ignition switch to ACC (I). The shift lever must be in the P position. Disconnect the steering lock assembly connector. Check if the ignition key can be moved to LOCK (0) position, and remove the key from the cylinder. Is the ignition key able to move to the LOCK (0) position, and then removed?
YES | - | Go to Step 4 .
NO | - | Replace the ignition key cylinder/steering lock assembly. ■
Turn the ignition switch to ACC (I) or ON (II), and shift to the N position. Check for the voltage between the No. 4 terminal of the steering lock assembly connector and body ground. Is there battery voltage?
YES | - | Go to Step 6 .
NO | - | Check for an open in with WHT/BLU wire between the MICU and the steering lock assembly connector. If the wire is OK, substitute a known-good multiplex integrated control unit and recheck.■
Turn the ignition switch to ACC (I), and shift to the P position. Remove the center console. Disconnect the transmission gear selection switch/park pin switch connector. |