Without the HDS Make sure you have the anti-theft codes for the radio, and Navigation if equipped then write down the frequencies for the radio's preset buttons. Remove the left kick panel, then remove PGM-Fl main relay 2 (FUEL PUMP) (A) from the under-dash fuse/relay box. Start the engine, and let it idle until it stalls. NOTE: If any DTCs are stored, clear and ignore them. Turn the ignition switch OFF. Remove the fuel fill cap, and relieve the pressure in the fuel tank. Disconnect the negative cable from the battery. |