LKAS Control Unit DTC 25: A/T (PGM-FI ECU) Malfunction Clear the DTC using the HDS. Turn the ignition switch OFF, then turn it ON (II). Watch the D indicator in the gauge control module. Does the blink?
YES | - | Go to Step 4 .
NO | - | Intermittent failure, the system is OK at this time.■
Check for LKAS control unit DTCs with HDS. Is DTC indicated?
YES | - | Do the troubleshoot for the A/T system. ■
NO | - | Troubleshoot the indicated DTC.■