Starter

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Starter | Output |  | 2.0 kW
Commutator mica depth |  | 0.5 mm (0.020 in.) | 0.20 mm (0.008 in.)
Commutator runout |  | 0.05 mm (0.002 in.) max. | 0.1 mm (0.004 in.)
Commutator O.D. |  | 31.9−32.1 mm (1.256−1.263 in.) | 31.4 mm (1.24 in.)
Brush length |  | 18.0 mm (0.7 in.) | 11.0 mm (0.4 in.)