NOTE: Check the weatherstrips and glass run channel for damage or deterioration, and replace them if necessary. Wipe the run channel clean with a shop towel. Lubricate the run channel with Shin-Etsu silicone grease P/N 08798-9013. Place the vehicle on a firm, level surface. Remove these items: Door panel, front door, rear door Plastic cover, front door, rear door Carefully move the glass (A) until you can see the glass mounting bolts (B), then loosen them. Push the glass against the channel (C), then tighten the glass mounting bolts. Make sure that the glass moves smoothly. | Front door Rear door