Maintenance Schedule for Normal Conditions

Follow the Normal Conditions Maintenance Schedule if the severe driving conditions specified in the Severe Conditions Maintenance Schedule do not apply.

Service at the indicated distance or time whichever comes first | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200 | 220 | 240
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12.5 | 25.0 | 37.5 | 50.0 | 62.5 | 75.0 | 87.5 | 100.0 | 112.5 | 125.0 | 137.5 | 150.0
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120 | 132 | 144
Replace engine oil | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Replace engine oil filter | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Replace air cleaner element | Every 40,000 km (25,000 miles)
Drain fuel filter | ● |  | ● |  | ● |  | ● |  | ● |  | ● |
Replace fuel filter |  | ● |  | ● |  | ● |  | ● |  | ● |  | ●
Inspect drive belts Check for cracks and damage Check deflection and tension
Replace engine coolant Use genuine Honda All Season Antifreeze/ Coolant Type 2 |  |  |  |  | ● |  |  | ● |  |  | ● |
Replace manual transmission fluid Use genuine Honda MTF | Every 120,000 km (75,000 miles) or 8 years
Inspect front and rear brakes Check the brake pad and disc thickness. Check for damage or cracks front pad, front disc, rear pad, rear disc Check the brake linings for cracking, grazing, wear, and contamination Check the calipers for damage, leaks, and tightness | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Replace brake fluid Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid Check that brake fluid level between the upper and lower marks on the reservoir | Every 3 years
Check parking brake adjustment Check the parking brake operation | ● | ● |  | ● |  | ● |  | ● |  | ● |  | ●
Replace dust and pollen filter Replace every 20,000 km (12,500 miles) or 1 year when the customer drives primarily in urban areas that have high concentrations of soot in the air, under dusty conditions, or the air flow from the heating and cooling system becomes less than normal. |  | ● |  | ● |  | ● |  | ● |  | ● |  | ●

Service at the indicated distance or time whichever comes first | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200 | 220 | 240
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12.5 | 25.0 | 37.5 | 50.0 | 62.5 | 75.0 | 87.5 | 100.0 | 112.5 | 125.0 | 137.5 | 150.0
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120 | 132 | 144
Check lights alignment Check the position of the headlights | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Check expiry date for temporary repair kit bottle
Test drive (noise, stability, dashboard operation)
Inspect vehicle corrosion: refer to the Body Repair Manual External Paintwork and panel Corrosion Check Under body Corrosion Check | Every year
Visually inspect the following items: Check for correct installation and position, check for cracks, deterioration, rust, and leaks Check tightness of screws, nuts, and joints. If necessary, retighten
Tie-rod ends, steering gearbox, and boots Check rack grease and steering linkage. Check the boot for damage and leaking grease | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Suspension components Check the bolts for tightness Check all dust cover for deterioration and damage
Driveshaft boots Check the boot and boot band for cracks Check rack grease
Brake hoses and lines (including VSA) Check the master cylinder and VSA modulator-control unit and leakage
All fluid levels and condition of fluids Check levels and check for leaks. If necessary, add engine coolant, MTF, brake fluid, power steering fluid , andwindshield fluid
Exhaust system Check the catalytic converter heat shield, exhaust pipe, and muffler for damage, leaks, and tightness
Fuel lines and connections Check fuel lines for loose connections, cracks, and deterioration. Retighten loose connections and replace any damaged parts
Tyre condition