Remove the cam chain. Loosen the rocker arm adjusting screws. Remove the camshaft holder. Remove the intake camshaft. Check that the variable valve timing control (VTC) actuator is locked by turning the VTC actuator clockwise and counterclockwise. If the VTC actuator is not locked, replace the VTC actuator. Seal the advance holes (A) and retard holes (B) in the No. 1 camshaft journal with the tape. Punch a hole in the tape over one of the advance holes. |