DTC 33-8x (33-80 to 33-89, 33-8A to 33-8F): Short to Power in Left Side Curtain Airbag Inflator Special Tools Required SRS inflator simulator 07SAZ-TB4011A SRS simulator lead E 07XAZ-S1A0200 Erase the DTC memory. Turn the ignition switch ON (II), and check that the SRS indicator comes on for about 6 seconds and then goes off. Does the SRS indicator stay on and is DTC 33-8x indicated?
YES | - | Go to Step 3 .
NO | - | Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures. If another DTC is indicated, go to the DTC troubleshooting index for troubleshooting details.
Turn the ignition switch OFF. Disconnect the battery negative cable, and wait for 3 minutes. Disconnect the left side curtain airbag 2P connector from the side curtain airbag subharness (A). Connect the SRS inflator simulator (2 Ω connector) and simulator lead E to side curtain airbag subharness. Reconnect the battery negative cable. Erase the DTC memory. Read the DTC. Is DTC 33-8x indicated?
YES | - | Go to Step 9 .
NO | - | Short to power in the left side curtain airbag inflator; replace the left side curtain airbag. ■
Turn the ignition switch OFF. Disconnect the battery negative cable, and wait for 3 minutes. |