Maintenance Schedule for Normal and Severe Conditions - Except EU
37,000miles(3year)

This Maintenance Schedule outlines the minimum required maintenance that you should perform to ensure the trouble-free operation of the vehicle. Due to regional and climatic differences, some additional service may be required. Please consult the warranty booklet for a more detalied description.
The following items must be used for ‘‘severe conditions'' indicated on schedule, if the vehicle is driven MAINLY under the specified conditions A to E.

- Engine oil and engine oil filter: A/B/C/D/E
- Air cleaner element: D/E
- Transmission fluid: B/D

A: Driving less than 8 km (5 miles) per trip or, in freezing temperatures, driving less than 16 km (10 miles) per trip.
B: Driving in extremely hot over 35 °C (95 °F) conditions.
C: Extensive idling, or long periods of stop-and-go driving.
D: Trailer towing, driving with a loaded roof rack, or driving in mountainous conditions.
E: Driving on muddy, dusty, or de-iced roads.

Service at the indicated distance or time whichever comes first

| Replace air cleaner element

| Replace fuel filter
Replace fuel filter every 40,000 km (25,000 miles) or 2 years, if the fuel the customer uses is suspected to be contaminated.

| Replace Manual Transmission Fluid (MTF)
Use genuine Honda MTF.

| Replace dust and pollen filter

| Brake hoses and lines (including VSA lines)
Check the master cylinder and VSA modulator-control unit and leakage.

| All fluid levels and condition of fluid
Check levels and check for leaks. If necessary, add.
|  | Engine coolant
|  | MTF
|  | Clutch fluid
|  | Power steering fluid
|  | Brake fluid
|  | Windshield fluid

| Exhaust system
Check the catalytic converter heat shield, exhaust pipe, and muffler for damage, leaks, and tightness.

| Fuel lines and connections
|  | Check fuel lines for loose connections, cracks, and deterioration.
|  | Retighten loose connections and replace any damaged parts.

Every 10,000 km (6,250 miles) or 1 year

| Replace engine oil and filter

Every 5,000 km (3,125 miles) or 6 months

| Replace engine oil and filter

Every 10,000 km (6,250 miles)

| Replace air cleaner element

| Rotate tyres
Check tyre inflation at least once per month.

Every 10,000 km (6,250 miles) or 6 months

| Check front and rear brakes
Check the brake pad and disc thickness. Check for damage or cracks.

| Tie-rod ends, steering gearbox, and boots
|  | Check rack grease and steering linkage.
|  | Check the boot for damage and leaking grease.

| Suspension components
|  | Check the bolts for tightness.
|  | Check all dust covers for deterioration and damage.

| Driveshaft boots
|  | Check the boot and boot band for cracks.
|  | Check rack grease.

Every 3 years

| Replace brake fluid
|  | Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid.
|  | Check the brake fluid level is between the upper and lower marks on the reservoir.