Clutch - 4/4

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Clutch - 4/4 | 1st clutch end-plate thickness (K24A3) | Mark F or Q | 2.6 mm (0.102 in.) | When discolored
Mark G or R | 2.7 mm (0.106 in.) | When discolored
Mark H or S | 2.8 mm (0.110 in.) | When discolored
Mark J or T | 2.9 mm (0.114 in.) | When discolored
Mark K or U | 3.0 mm (0.118 in.) | When discolored
Mark L or V | 3.1 mm (0.122 in.) | When discolored
Mark M or W | 3.2 mm (0.126 in.) | When discolored
Mark N or X | 3.3 mm (0.130 in.) | When discolored
Mark P or Y | 3.4 mm (0.134 in.) | When discolored
2nd clutch end-plate thickness (K24A3) | Mark 10 | 2.4 mm (0.094 in.) | When discolored
Mark 11 | 2.5 mm (0.098 in.) | When discolored
Mark 1 | 2.6 mm (0.102 in.) | When discolored
Mark 2 | 2.7 mm (0.106 in.) | When discolored
Mark 3 | 2.8 mm (0.110 in.) | When discolored
Mark 4 | 2.9 mm (0.114 in.) | When discolored
Mark 5 | 3.0 mm (0.118 in.) | When discolored
Mark 6 | 3.1 mm (0.122 in.) | When discolored
Mark 7 | 3.2 mm (0.126 in.) | When discolored
3rd clutch end-plate thickness (K24A3) | Mark BA or BK | 2.2 mm (0.086 in.) | When discolored
Mark BB or BL | 2.3 mm (0.090 in.) | When discolored
Mark BC or BM | 2.4 mm (0.094 in.) | When discolored
Mark BD or BN | 2.5 mm (0.098 in.) | When discolored
Mark BE or BP | 2.6 mm (0.102 in.) | When discolored
Mark BF or BQ | 2.7 mm (0.106 in.) | When discolored
Mark BG or BR | 2.8 mm (0.110 in.) | When discolored
Mark BH or BS | 2.9 mm (0.114 in.) | When discolored
Mark BJ or BT | 3.0 mm (0.118 in.) | When discolored
4th, 5th clutch end-plate thickness (K24A3) | Mark 1 | 2.1 mm (0.082 in.) | When discolored
Mark 2 | 2.2 mm (0.086 in.) | When discolored
Mark 3 | 2.3 mm (0.090 in.) | When discolored
Mark 4 | 2.4 mm (0.094 in.) | When discolored
Mark 5 | 2.5 mm (0.098 in.) | When discolored
Mark 6 | 2.6 mm (0.102 in.) | When discolored
Mark 7 | 2.7 mm (0.106 in.) | When discolored
Mark 8 | 2.8 mm (0.110 in.) | When discolored
Mark 9 | 2.9 mm (0.114 in.) | When discolored