Back-up Light Switch Test

Make sure you have the anti-theft codes for the audio and the navigation system, then write down the frequencies for the audio preset buttons. Disconnect the negative (−) cable first, then the positive (+) cable from the battery. Remove the battery. Remove the air cleaner housing. Remove the battery base. Remove the intake air cover. |

Remove the resonator chamber. |

Disconnect the back-up light switch connector (A). Check for continuity between the No. 1 and No. 2 terminals of the back-up light switch 2P connector. There should be continuity when the shift lever is in reverse. If necessary, replace the back-up light switch. Apply liquid gasket (P/N 08C70-K0234M) to the switch threads, and install the switch on the transmission housing. Tighten the back-up light switch to the specified torque. Install the resonator chamber. Install the battery base, then install the ground cable. Install the air cleaner housing. Install the battery. Connect the positive (+) cable first, then the negative (−) cable to the battery. Enter the anti-theft codes for the audio and navigation system, then enter the customer's audio presets. Do the power window control unit reset procedure. |