NOTE: Do not use this troubleshooting procedure if the radiator fan and/or the A/C compressor is inoperative. Refer to the symptom troubleshooting index. Before performing symptom troubleshooting, check for powertrain DTCs. Check the No. 30 (7.5 A) fuse in the under-dash fuse/relay box. Is the fuse OK?
YES | - | Go to Step 2 .
NO | - | Replace the fuse, and recheck.■
Remove the fan control relay from the multi-relay box, and test it. Is the relay OK?
YES | - | Go to Step 3 .
NO | - | Replace the fan control relay.■
Turn the ignition switch ON (II). Measure the voltage between the No. 5 terminal of the fan control relay 5P socket and body ground. Is there battery voltage?
YES | - | Go to Step 5 .
NO | - | Go to Step 17 .
Turn the ignition switch OFF. |