1. NOTE: Do not rotate the camshaft during inspection. Remove the rocker arm assembly. Put the rocker shaft holders, camshaft, and camshaft holders on the cylinder head, then tighten the bolts to the specified torque. Specified Torque
   8 mm Bolts: | 22 N·m (2.2 kgf·m, 16 lbf·ft)
   6 mm Bolts: | 12 N·m (1.2 kgf·m, 8.7 lbf·ft)
   6 mm Bolts: (21), (22), (23)
Seat the camshaft by pushing it away from the camshaft pulley end of the cylinder head. |