Connect the No. 1 terminal of the A/C condenser fan 2P connector to body ground with jumper wire. Turn the ignition switch ON (II), then turn the A/C and fan switches ON. Does the A/C condenser fan run?
YES | - | Go to Step 29 .
NO | - | Replace the A/C condenser fan motor.■
Turn the A/C and fan switches OFF, then turn the ignition switch OFF. Disconnect the jumper wire. Remove the fan control relay from the multi-relay box, and test it. Is the relay OK?
YES | - | Go to Step 32 .
NO | - | Replace the fan control relay.■
Turn the ignition switch ON (II), then turn the A/C and fan switches ON. |