DTC P0563: ECM/PCM Power Source Circuit Unexpected Voltage NOTE: Information marked with an asterisk ( * ) applies to RHD model. Turn the ignition switch ON (II). Clear the DTC with the HDS. Turn the ignition switch OFF. Wait 10 seconds. Turn the ignition switch ON (II). Check for Temporary DTCs or DTCs with the HDS. Is DTC P0563 indicated?
YES | - | Go to Step 7 .
NO | - | Intermittent failure, system is OK at this time. Check for poor connections or loose terminals at the No. 8 FI ECU (ECM/PCM) (15 A) fuse in the under-hood fuse/relay box, PGM-FI main relay 1 (FI MAIN) and the ECM/PCM.■
Turn the ignition switch OFF. Jump the SCS line with the HDS. Disconnect ECM/PCM connector E (31P). Measure voltage between ECM/PCM connector terminal E7 and body ground. Is there battery voltage?
YES | - | Go to Step 13 .
NO | - | Go to Step 11 .