DTC B1376: Power Tailgate Outer Handle Switch Signal Error Clear the DTCs using the HDS. Cycle the ignition switch to OFF, and then back ON. After 2 secons or more, pull the tailgate outer handle 2 seconds or more. Check for DTCs by the DTCs MENU (DTCs) from the HDS. Is DTC B1376 indicated?
YES | - | Go to Step 5 .
NO | - | Intermittent failure, the system is OK at this time.■
Cycle the ignition swith to OFF. Open the tailgate fully with the transmitter. Disconnect connector A (26P) from the power tailgate control unit. Check for continuity between the No. 10 and No. 12 terminals of power tailgate control unit connector A (26P) and body ground. Is there continuity?
YES | - | Repair a short in the WHT/RED (OHSW) or YEL/BLK (SCOM) wire.■
NO | - | Go to Step 9 .