Install a new spindle nut (A), then tighten the nut. After tightening, use a drift to stake the spindle nut shoulder (B) against the driveshaft. Clean the mating surfaces of the brake disc and the front wheel, then install the front wheel with the wheel nuts. Turn the front wheel by hand, and make sure the clearance between the driveshaft and circumference parts. Tighten the flange bolt and the self-locking nut with the vehicle's weight on the damper. Refill the transmission with recommended transmission fluid: Manual transmission Automatic transmission Check the front wheel alignment, and adjust it if necessary. |