Measure the voltage between engine mount control solenoid valve 2P connector terminals No. 1 and No. 2. Is there battery voltage?
YES | - | Repair a short to body ground in the wire between ECM/PCM (B15) and the engine mount control solenoid valve. If the wire is OK, update the ECM/PCM if it does not have the latest software, or substitute a known-good ECM/PCM, and recheck. If the engine mount control system works properly, and the ECM/PCM was updated, the troubleshooting is complete. If the ECM/PCM was substituted, replace the original ECM/PCM. ■
NO | - | Go to Step 10 .