Automatic Dimming Inside Mirror Test/Replacement

1. Remove the automatic dimming inside mirror cover. Disconnect the 7P connector (A) from the automatic inside dimming mirror (B). Check for continuity between No. 2 terminal and body ground. If there is continuity, go to Step 4 . If there is no continuity, check for:
   - | An open in the wire.
   - | Poor ground (G501 (LHD), G601 (RHD)).
1. Check for voltage between No. 1 terminal and body ground with the ignition switch ON (II). If there is battery voltage, go to Step 5 . If there is no voltage, check for:
   - | Blown No. 21 (7.5 A) fuse in the driver's under-dash fuse/relay box.
   - | An open in the wire.
1. Check for voltage between No. 3 terminal and body ground with the ignition switch turned ON (II) and transmission range switch (A/T) or back-up light switch (M/T) in reverse. If there is battery voltage, replace the mirror assembly. If there is no voltage, check for:
   - | An open in the wire.
   - | Blown No. 21 (7.5 A) fuse in the under-dash fuse/relay box.
   - | Faulty reverse relay.
   - | Faulty transmission range switch .