Check for continuity between the adaptive cruise control (ACC) unit 20P connector No. 5 terminal and body ground. Is there about 5 V?
YES | - | Go to Step 12 .
NO | - | Repair a short to ground in the wire between the adaptive cruise control (ACC) unit and the right front pressure sensor.■
Remove the jumper wire from the right front pressure sensor. Reconnect all connectors. Turn the ignition switch ON (II). |