VSA activation indicator does not go off, and no DTCs are stored Turn the ignition switch ON (II), and watch the VSA indicator. Does the VSA indicator go off?
YES | - | Go to Step 2 .
NO | - | Do the appropriate troubleshooting for the VSA indicator.■
Turn the ignition switch OFF. Check the VSA OFF switch. Is the switch OK?
YES | - | Go to Step 4 .
NO | - | Replace the VSA OFF switch. ■
Clear the DTC using the HDS. Does the VSA activation indicator go off?
YES | - | The system is OK at this time.■
NO | - | Go to Step 5 .
Do the VSA sensor neutral memorization. Clear the DTC using the HDS. Does the VSA activation indicator go off?
YES | - | The system is OK at this time.■
NO | - | Go to Step 7 .
Remove the gauge control module. Check for continuity between the VSA OFF switch 5P connector terminal No. 2 and body ground. Is there continuity?
YES | - | Repair short to body ground in the wire between the gauge control module and the VSA OFF switch.■
NO | - | Go to Step 9 .