how to fix rcc ip logging

1. open rcc in x32dbg
2. go to symbols
3. select ur rcc
4. az / a2 button
5. search connection accepted
6. double click on it
7. right click -> follow in dump -> rcc.randomnumbersandletters
8. select search connection accepted.. in dump (the main thing is %s)
9. press ctrl + e
10. replace %s to something like no
11. string search for new connection from
12. click new connection from %s
13. do the same thing as with the previous one, %s is the part where the ip is being put

enjoy!!