1. Remove the power window switch panel (A).

   -1. | Pry up on the rear edge (driver's) or front edge (passenger's) of the switch panel with a flat-tip screwdriver wrapped with protective tape to release the rear clip.
   -2. | Pull out along the edge of the panel to release the hooks (B) and front clip.
   -3. | Disconnect the power mirror switch connector (C) (driver's) and the power window switch connector (D).

Driver's
Passenger's