SRS Unit, Front Impact Sensors and Side Impact Sensors

- Be careful not to bump or impact the SRS unit, front impact sensors or the side impact sensors whenever the ignition switch is ON (II), or for at least 3 minutes after the ignition switch is turned OFF.
- During installation or replacement, be careful not to bump (by impact wrench, hammer, etc.) the area around the SRS unit, front impact sensors, and the side impact sensor. The airbags could accidentally deploy and cause damage or injury.