Fuse to Components Index - Under-dash Fuse/Relay Box

Under-dash Fuse/Relay Box

Fuse Number | Amps | Wire Color | Component (s) or Circuit (s) Protected
--- | --- | --- | ---
1 | 15 A | WHT/BLU | Throttle actuator control module
2 | 15 A | ——— | Ignition coil relay
BLK/WHT | Ignition coils
3 | ——— | ——— | Not used
4 | 10 A | BLU/WHT | Air/fuel ratio sensor
5 | 20 A | WHT/GRN | Audio unit (+B), Hands free telephone control unit
6 | 10 A | WHT/BLU | Driver's door courtesy light, Front passenger's door courtesy light, Individual map lights, Driver's vanity mirror light, Passenger's vanity mirror light, Ceiling light (With sunroof), Audio unit (+B), Right cargo area light, Left cargo area light, Power tailgate inner switch light
7 | 10 A | WHT | Combination switch control unit, Gauge control module, Immobilizer control unit-receiver, Immoes control unit, Navigation display unit, Navigation unit, Power tailgate control unit, Ultrasonic sensor, Alarm control siren, Automatic lighting control unit
——— | Multiplex integrated control unit
8 | 20 A | RED/YEL | Multiplex integrated control unit (+B door lock)
9 | 15 A | WHT/RED | Cigarette lighter
10 | 7.5 A | WHT | SRS unit, OPDS unit
11 | 30 A | GRN | Windshield wiper motor
12 | 10 A | RED/BLU | Rear accessory power socket
13 | 7.5 A | RED/YEL | Rear fog light
14 | 20 A | WHT/BLU | Driver's power seat slide motor
15 | 20 A | RED/BLK | Seat heater and indicator
16 | 20 A | WHT/RED | Driver's power seat recline motor
17 | 20 A | WHT/ORN | Front passenger's power seat slide motor
18 | 15 A | BLK/RED | ELD unit, Secondary HO2S, Alternator, Cruise control unit, CAM sensor, Engine mount control solenoid (A/T)
19 | 15 A | BLK/YEL | ECM/PCM, Immobilizer control unit receiver, Immoes control unit
YEL/GRN | Fuel pump
20 | 7.5 A | YEL/GRN | Windshield washer motor, Headlight adjuster units, Headlight adjuster switch, Rear window wiper motor, Rear window wiper motor relay, Rear window washer motor, Rear window washer motor relay, Rain sensor, Sunroof open relay, Sunroof close relay
21 | 10 A | YEL | Gauge control module, A/T shift lock solenoid, Back-up lights, Door multiplex control unit, Keyless receiver unit, Power tailgate control unit, Automatic dimming inside mirror, Automatic lighting control unit
——— | Combination switch control unit, Multiplex integrated control unit, Door multiplex control unit
22 | 10 A | WHT/RED | SRS unit
23 | 7.5 A | ORN | ECM/PCM (LAF R)
24 | 20 A | YEL/RED | Left power window motor
25 | 20 A | YEL/BLU | Right power window motor
26 | 20 A | GRN/BLK | Front passenger's power window motor
27 | 20 A | GRN/WHT | Driver's power window motor
28 | 20 A | GRN | Sunroof motor
29 | 7.5 A | YEL/BLU | Headlight adjuster unit, Headlight adjuster switch light, Headlight adjuster control unit, Adaptive cruise control unit, Headlight adjuster unit
30 | 7.5 A | * | Power mirror actuators, Power mirror defogger, Climate control unit, Recirculation control motor, Seat heater relay
BLK/YEL | Rear window defogger relay, Blower motor relay, Radiator fan relay, condenser fan relay, A/C compressor clutch relay, ECM/PCM (ACC), ECM/PCM (FANC)
31 | 7.5 A | —— | LKAS unit (KE model with adaptive cruise control)
32 | 7.5 A | RED | Audio unit (ACC), Navigation display unit, Navigation unit, Rear accessory power socket relay, Accessory power socket relay (KE model), Hands free telephone control unit
——— | Cigarette lighter relay
33 | —— | —— | Not used

* | LHD: | WHT
| RHD: | BLK/YEL